SNMPv2-TM DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-IDENTITY,
    snmpModules, snmpDomains, snmpProxys
        FROM SNMPv2-SMI
    TEXTUAL-CONVENTION
        FROM SNMPv2-TC;

snmpv2tm MODULE-IDENTITY
    LAST-UPDATED "200210160000Z"
    ORGANIZATION "IETF SNMPv3 Working Group"
    CONTACT-INFO
            "WG-EMail:   snmpv3@lists.tislabs.com
             Subscribe:  snmpv3-request@lists.tislabs.com

             Co-Chair:   Russ Mundy
                         Network Associates Laboratories
             postal:     15204 Omega Drive, Suite 300
                         Rockville, MD 20850-4601
                         USA
             EMail:      mundy@tislabs.com
             phone:      +1 301 947-7107



             Co-Chair:   David Harrington
                         Enterasys Networks
             postal:     35 Industrial Way
                         P. O. Box 5005
                         Rochester, NH 03866-5005
                         USA
             EMail:      dbh@enterasys.com
             phone:      +1 603 337-2614

             Editor:     Randy Presuhn
                         BMC Software, Inc.
             postal:     2141 North First Street
                         San Jose, CA 95131
                         USA
             EMail:      randy_presuhn@bmc.com
             phone:      +1 408 546-1006"
    DESCRIPTION
            "The MIB module for SNMP transport mappings.

             Copyright (C) The Internet Society (2002). This
             version of this MIB module is part of RFC 3417;
             see the RFC itself for full legal notices.
            "
    REVISION     "200210160000Z"
    DESCRIPTION
            "Clarifications, published as RFC 3417."
    REVISION    "199601010000Z"
    DESCRIPTION
            "Clarifications, published as RFC 1906."
    REVISION    "199304010000Z"
    DESCRIPTION
            "The initial version, published as RFC 1449."
    ::= { snmpModules 19 }

-- SNMP over UDP over IPv4

snmpUDPDomain  OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The SNMP over UDP over IPv4 transport domain.
            The corresponding transport address is of type
            SnmpUDPAddress."
    ::= { snmpDomains 1 }








SnmpUDPAddress ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "1d.1d.1d.1d/2d"
    STATUS       current
    DESCRIPTION
            "Represents a UDP over IPv4 address:

               octets   contents        encoding
                1-4     IP-address      network-byte order
                5-6     UDP-port        network-byte order
            "
    SYNTAX       OCTET STRING (SIZE (6))

-- SNMP over OSI

snmpCLNSDomain OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The SNMP over CLNS transport domain.
            The corresponding transport address is of type
            SnmpOSIAddress."
    ::= { snmpDomains 2 }

snmpCONSDomain OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The SNMP over CONS transport domain.
            The corresponding transport address is of type
            SnmpOSIAddress."
    ::= { snmpDomains 3 }

SnmpOSIAddress ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "*1x:/1x:"
    STATUS       current
    DESCRIPTION
            "Represents an OSI transport-address:

          octets   contents           encoding
             1     length of NSAP     'n' as an unsigned-integer
                                         (either 0 or from 3 to 20)
          2..(n+1) NSAP                concrete binary representation
          (n+2)..m TSEL                string of (up to 64) octets
            "
    SYNTAX       OCTET STRING (SIZE (1 | 4..85))








-- SNMP over DDP

snmpDDPDomain  OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The SNMP over DDP transport domain.  The corresponding
            transport address is of type SnmpNBPAddress."
    ::= { snmpDomains 4 }

SnmpNBPAddress ::= TEXTUAL-CONVENTION
    STATUS       current
    DESCRIPTION
            "Represents an NBP name:

         octets        contents          encoding
            1          length of object  'n' as an unsigned integer
          2..(n+1)     object            string of (up to 32) octets
           n+2         length of type    'p' as an unsigned integer
      (n+3)..(n+2+p)   type              string of (up to 32) octets
          n+3+p        length of zone    'q' as an unsigned integer
    (n+4+p)..(n+3+p+q) zone              string of (up to 32) octets

            For comparison purposes, strings are
            case-insensitive. All strings may contain any octet
            other than 255 (hex ff)."
    SYNTAX       OCTET STRING (SIZE (3..99))

-- SNMP over IPX

snmpIPXDomain  OBJECT-IDENTITY
    STATUS     current
    DESCRIPTION
            "The SNMP over IPX transport domain.  The corresponding
            transport address is of type SnmpIPXAddress."
    ::= { snmpDomains 5 }

SnmpIPXAddress ::= TEXTUAL-CONVENTION
    DISPLAY-HINT "4x.1x:1x:1x:1x:1x:1x.2d"
    STATUS       current
    DESCRIPTION
            "Represents an IPX address:

               octets   contents            encoding
                1-4     network-number      network-byte order
                5-10    physical-address    network-byte order
               11-12    socket-number       network-byte order
            "
    SYNTAX       OCTET STRING (SIZE (12))



-- for proxy to SNMPv1 (RFC 1157)

rfc1157Proxy   OBJECT IDENTIFIER ::= { snmpProxys 1 }

rfc1157Domain  OBJECT-IDENTITY
    STATUS     deprecated
    DESCRIPTION
            "The transport domain for SNMPv1 over UDP over IPv4.
            The corresponding transport address is of type
            SnmpUDPAddress."
    ::= { rfc1157Proxy 1 }

--  ::= { rfc1157Proxy 2 }            this OID is obsolete

END
